\documentclass[11pt,twoside]{article}\makeatletter

\IfFileExists{xcolor.sty}%
  {\RequirePackage{xcolor}}%
  {\RequirePackage{color}}
\usepackage{colortbl}
\usepackage{wrapfig}
\usepackage{ifxetex}
\ifxetex
  \usepackage{fontspec}
  \usepackage{xunicode}
  \catcode`⃥=\active \def⃥{\textbackslash}
  \catcode`❴=\active \def❴{\{}
  \catcode`❵=\active \def❵{\}}
  \def\textJapanese{\fontspec{Noto Sans CJK JP}}
  \def\textChinese{\fontspec{Noto Sans CJK SC}}
  \def\textKorean{\fontspec{Noto Sans CJK KR}}
  \setmonofont{DejaVu Sans Mono}
  
\else
  \IfFileExists{utf8x.def}%
   {\usepackage[utf8x]{inputenc}
      \PrerenderUnicode{–}
    }%
   {\usepackage[utf8]{inputenc}}
  \usepackage[english]{babel}
  \usepackage[T1]{fontenc}
  \usepackage{float}
  \usepackage[]{ucs}
  \uc@dclc{8421}{default}{\textbackslash }
  \uc@dclc{10100}{default}{\{}
  \uc@dclc{10101}{default}{\}}
  \uc@dclc{8491}{default}{\AA{}}
  \uc@dclc{8239}{default}{\,}
  \uc@dclc{20154}{default}{ }
  \uc@dclc{10148}{default}{>}
  \def\textschwa{\rotatebox{-90}{e}}
  \def\textJapanese{}
  \def\textChinese{}
  \IfFileExists{tipa.sty}{\usepackage{tipa}}{}
\fi
\def\exampleFont{\ttfamily\small}
\DeclareTextSymbol{\textpi}{OML}{25}
\usepackage{relsize}
\RequirePackage{array}
\def\@testpach{\@chclass
 \ifnum \@lastchclass=6 \@ne \@chnum \@ne \else
  \ifnum \@lastchclass=7 5 \else
   \ifnum \@lastchclass=8 \tw@ \else
    \ifnum \@lastchclass=9 \thr@@
   \else \z@
   \ifnum \@lastchclass = 10 \else
   \edef\@nextchar{\expandafter\string\@nextchar}%
   \@chnum
   \if \@nextchar c\z@ \else
    \if \@nextchar l\@ne \else
     \if \@nextchar r\tw@ \else
   \z@ \@chclass
   \if\@nextchar |\@ne \else
    \if \@nextchar !6 \else
     \if \@nextchar @7 \else
      \if \@nextchar (8 \else
       \if \@nextchar )9 \else
  10
  \@chnum
  \if \@nextchar m\thr@@\else
   \if \@nextchar p4 \else
    \if \@nextchar b5 \else
   \z@ \@chclass \z@ \@preamerr \z@ \fi \fi \fi \fi
   \fi \fi  \fi  \fi  \fi  \fi  \fi \fi \fi \fi \fi \fi}
\gdef\arraybackslash{\let\\=\@arraycr}
\def\@textsubscript#1{{\m@th\ensuremath{_{\mbox{\fontsize\sf@size\z@#1}}}}}
\def\Panel#1#2#3#4{\multicolumn{#3}{){\columncolor{#2}}#4}{#1}}
\def\abbr{}
\def\corr{}
\def\expan{}
\def\gap{}
\def\orig{}
\def\reg{}
\def\ref{}
\def\sic{}
\def\persName{}\def\name{}
\def\placeName{}
\def\orgName{}
\def\textcal#1{{\fontspec{Lucida Calligraphy}#1}}
\def\textgothic#1{{\fontspec{Lucida Blackletter}#1}}
\def\textlarge#1{{\large #1}}
\def\textoverbar#1{\ensuremath{\overline{#1}}}
\def\textquoted#1{‘#1’}
\def\textsmall#1{{\small #1}}
\def\textsubscript#1{\@textsubscript{\selectfont#1}}
\def\textxi{\ensuremath{\xi}}
\def\titlem{\itshape}
\newenvironment{biblfree}{}{\ifvmode\par\fi }
\newenvironment{bibl}{}{}
\newenvironment{byline}{\vskip6pt\itshape\fontsize{16pt}{18pt}\selectfont}{\par }
\newenvironment{citbibl}{}{\ifvmode\par\fi }
\newenvironment{docAuthor}{\ifvmode\vskip4pt\fontsize{16pt}{18pt}\selectfont\fi\itshape}{\ifvmode\par\fi }
\newenvironment{docDate}{}{\ifvmode\par\fi }
\newenvironment{docImprint}{\vskip 6pt}{\ifvmode\par\fi }
\newenvironment{docTitle}{\vskip6pt\bfseries\fontsize{22pt}{25pt}\selectfont}{\par }
\newenvironment{msHead}{\vskip 6pt}{\par}
\newenvironment{msItem}{\vskip 6pt}{\par}
\newenvironment{rubric}{}{}
\newenvironment{titlePart}{}{\par }

\newcolumntype{L}[1]{){\raggedright\arraybackslash}p{#1}}
\newcolumntype{C}[1]{){\centering\arraybackslash}p{#1}}
\newcolumntype{R}[1]{){\raggedleft\arraybackslash}p{#1}}
\newcolumntype{P}[1]{){\arraybackslash}p{#1}}
\newcolumntype{B}[1]{){\arraybackslash}b{#1}}
\newcolumntype{M}[1]{){\arraybackslash}m{#1}}
\definecolor{label}{gray}{0.75}
\def\unusedattribute#1{\sout{\textcolor{label}{#1}}}
\DeclareRobustCommand*{\xref}{\hyper@normalise\xref@}
\def\xref@#1#2{\hyper@linkurl{#2}{#1}}
\begingroup
\catcode`\_=\active
\gdef_#1{\ensuremath{\sb{\mathrm{#1}}}}
\endgroup
\mathcode`\_=\string"8000
\catcode`\_=12\relax

\usepackage[a4paper,twoside,lmargin=1in,rmargin=1in,tmargin=1in,bmargin=1in,marginparwidth=0.75in]{geometry}
\usepackage{framed}

\definecolor{shadecolor}{gray}{0.95}
\usepackage{longtable}
\usepackage[normalem]{ulem}
\usepackage{fancyvrb}
\usepackage{fancyhdr}
\usepackage{graphicx}
\usepackage{marginnote}

\renewcommand{\@cite}[1]{#1}


\renewcommand*{\marginfont}{\itshape\footnotesize}

\def\Gin@extensions{.pdf,.png,.jpg,.mps,.tif}

  \pagestyle{fancy}

\usepackage[pdftitle={Development of Boundary Element Method in Polar Coordinate System for Elasticity Problems},
 pdfauthor={}]{hyperref}
\hyperbaseurl{}

	 \paperwidth210mm
	 \paperheight297mm
              
\def\@pnumwidth{1.55em}
\def\@tocrmarg {2.55em}
\def\@dotsep{4.5}
\setcounter{tocdepth}{3}
\clubpenalty=8000
\emergencystretch 3em
\hbadness=4000
\hyphenpenalty=400
\pretolerance=750
\tolerance=2000
\vbadness=4000
\widowpenalty=10000

\renewcommand\section{\@startsection {section}{1}{\z@}%
     {-1.75ex \@plus -0.5ex \@minus -.2ex}%
     {0.5ex \@plus .2ex}%
     {\reset@font\Large\bfseries}}
\renewcommand\subsection{\@startsection{subsection}{2}{\z@}%
     {-1.75ex\@plus -0.5ex \@minus- .2ex}%
     {0.5ex \@plus .2ex}%
     {\reset@font\Large}}
\renewcommand\subsubsection{\@startsection{subsubsection}{3}{\z@}%
     {-1.5ex\@plus -0.35ex \@minus -.2ex}%
     {0.5ex \@plus .2ex}%
     {\reset@font\large}}
\renewcommand\paragraph{\@startsection{paragraph}{4}{\z@}%
     {-1ex \@plus-0.35ex \@minus -0.2ex}%
     {0.5ex \@plus .2ex}%
     {\reset@font\normalsize}}
\renewcommand\subparagraph{\@startsection{subparagraph}{5}{\parindent}%
     {1.5ex \@plus1ex \@minus .2ex}%
     {-1em}%
     {\reset@font\normalsize\bfseries}}


\def\l@section#1#2{\addpenalty{\@secpenalty} \addvspace{1.0em plus 1pt}
 \@tempdima 1.5em \begingroup
 \parindent \z@ \rightskip \@pnumwidth 
 \parfillskip -\@pnumwidth 
 \bfseries \leavevmode #1\hfil \hbox to\@pnumwidth{\hss #2}\par
 \endgroup}
\def\l@subsection{\@dottedtocline{2}{1.5em}{2.3em}}
\def\l@subsubsection{\@dottedtocline{3}{3.8em}{3.2em}}
\def\l@paragraph{\@dottedtocline{4}{7.0em}{4.1em}}
\def\l@subparagraph{\@dottedtocline{5}{10em}{5em}}
\@ifundefined{c@section}{\newcounter{section}}{}
\@ifundefined{c@chapter}{\newcounter{chapter}}{}
\newif\if@mainmatter 
\@mainmattertrue
\def\chaptername{Chapter}
\def\frontmatter{%
  \pagenumbering{roman}
  \def\thechapter{\@roman\c@chapter}
  \def\theHchapter{\roman{chapter}}
  \def\thesection{\@roman\c@section}
  \def\theHsection{\roman{section}}
  \def\@chapapp{}%
}
\def\mainmatter{%
  \cleardoublepage
  \def\thechapter{\@arabic\c@chapter}
  \setcounter{chapter}{0}
  \setcounter{section}{0}
  \pagenumbering{arabic}
  \setcounter{secnumdepth}{6}
  \def\@chapapp{\chaptername}%
  \def\theHchapter{\arabic{chapter}}
  \def\thesection{\@arabic\c@section}
  \def\theHsection{\arabic{section}}
}
\def\backmatter{%
  \cleardoublepage
  \setcounter{chapter}{0}
  \setcounter{section}{0}
  \setcounter{secnumdepth}{2}
  \def\@chapapp{\appendixname}%
  \def\thechapter{\@Alph\c@chapter}
  \def\theHchapter{\Alph{chapter}}
  \appendix
}
\newenvironment{bibitemlist}[1]{%
   \list{\@biblabel{\@arabic\c@enumiv}}%
       {\settowidth\labelwidth{\@biblabel{#1}}%
        \leftmargin\labelwidth
        \advance\leftmargin\labelsep
        \@openbib@code
        \usecounter{enumiv}%
        \let\p@enumiv\@empty
        \renewcommand\theenumiv{\@arabic\c@enumiv}%
	}%
  \sloppy
  \clubpenalty4000
  \@clubpenalty \clubpenalty
  \widowpenalty4000%
  \sfcode`\.\@m}%
  {\def\@noitemerr
    {\@latex@warning{Empty `bibitemlist' environment}}%
    \endlist}

\def\tableofcontents{\section*{\contentsname}\@starttoc{toc}}
\parskip0pt
\parindent1em
\def\Panel#1#2#3#4{\multicolumn{#3}{){\columncolor{#2}}#4}{#1}}
\newenvironment{reflist}{%
  \begin{raggedright}\begin{list}{}
  {%
   \setlength{\topsep}{0pt}%
   \setlength{\rightmargin}{0.25in}%
   \setlength{\itemsep}{0pt}%
   \setlength{\itemindent}{0pt}%
   \setlength{\parskip}{0pt}%
   \setlength{\parsep}{2pt}%
   \def\makelabel##1{\itshape ##1}}%
  }
  {\end{list}\end{raggedright}}
\newenvironment{sansreflist}{%
  \begin{raggedright}\begin{list}{}
  {%
   \setlength{\topsep}{0pt}%
   \setlength{\rightmargin}{0.25in}%
   \setlength{\itemindent}{0pt}%
   \setlength{\parskip}{0pt}%
   \setlength{\itemsep}{0pt}%
   \setlength{\parsep}{2pt}%
   \def\makelabel##1{\upshape ##1}}%
  }
  {\end{list}\end{raggedright}}
\newenvironment{specHead}[2]%
 {\vspace{20pt}\hrule\vspace{10pt}%
  \phantomsection\label{#1}\markright{#2}%

  \pdfbookmark[2]{#2}{#1}%
  \hspace{-0.75in}{\bfseries\fontsize{16pt}{18pt}\selectfont#2}%
  }{}
      \def\TheFullDate{2018-01-15 (revised: 15 January 2018)}
\def\TheID{\makeatother }
\def\TheDate{2018-01-15}
\title{Development of Boundary Element Method in Polar Coordinate System for Elasticity Problems}
\author{}\makeatletter 
\makeatletter
\newcommand*{\cleartoleftpage}{%
  \clearpage
    \if@twoside
    \ifodd\c@page
      \hbox{}\newpage
      \if@twocolumn
        \hbox{}\newpage
      \fi
    \fi
  \fi
}
\makeatother
\makeatletter
\thispagestyle{empty}
\markright{\@title}\markboth{\@title}{\@author}
\renewcommand\small{\@setfontsize\small{9pt}{11pt}\abovedisplayskip 8.5\p@ plus3\p@ minus4\p@
\belowdisplayskip \abovedisplayskip
\abovedisplayshortskip \z@ plus2\p@
\belowdisplayshortskip 4\p@ plus2\p@ minus2\p@
\def\@listi{\leftmargin\leftmargini
               \topsep 2\p@ plus1\p@ minus1\p@
               \parsep 2\p@ plus\p@ minus\p@
               \itemsep 1pt}
}
\makeatother
\fvset{frame=single,numberblanklines=false,xleftmargin=5mm,xrightmargin=5mm}
\fancyhf{} 
\setlength{\headheight}{14pt}
\fancyhead[LE]{\bfseries\leftmark} 
\fancyhead[RO]{\bfseries\rightmark} 
\fancyfoot[RO]{}
\fancyfoot[CO]{\thepage}
\fancyfoot[LO]{\TheID}
\fancyfoot[LE]{}
\fancyfoot[CE]{\thepage}
\fancyfoot[RE]{\TheID}
\hypersetup{citebordercolor=0.75 0.75 0.75,linkbordercolor=0.75 0.75 0.75,urlbordercolor=0.75 0.75 0.75,bookmarksnumbered=true}
\fancypagestyle{plain}{\fancyhead{}\renewcommand{\headrulewidth}{0pt}}

\date{}
\usepackage{authblk}

\providecommand{\keywords}[1]
{
\footnotesize
  \textbf{\textit{Index terms---}} #1
}

\usepackage{graphicx,xcolor}
\definecolor{GJBlue}{HTML}{273B81}
\definecolor{GJLightBlue}{HTML}{0A9DD9}
\definecolor{GJMediumGrey}{HTML}{6D6E70}
\definecolor{GJLightGrey}{HTML}{929497} 

\renewenvironment{abstract}{%
   \setlength{\parindent}{0pt}\raggedright
   \textcolor{GJMediumGrey}{\rule{\textwidth}{2pt}}
   \vskip16pt
   \textcolor{GJBlue}{\large\bfseries\abstractname\space}
}{%   
   \vskip8pt
   \textcolor{GJMediumGrey}{\rule{\textwidth}{2pt}}
   \vskip16pt
}

\usepackage[absolute,overlay]{textpos}

\makeatother 
      \usepackage{lineno}
      \linenumbers
      
\begin{document}

             \author[1]{Natela  Zirakashvili}

             \affil[1]{  I. Vekua Institute of Applied Mathematics of Iv. Javakhishvili Tbilisi State University}

\renewcommand\Authands{ and }

\date{\small \em Received: 13 December 2017 Accepted: 31 December 2017 Published: 15 January 2018}

\maketitle


\begin{abstract}
        


The article presents an exact version of the boundary element method, in particular, the fictitious load method used to solve boundary value and boundary-contact problems of elasticity. The method is developed in the polar coordinate system. The circular boundary of the area limited with the coordinate axes of this system is divided not into small segments like in case of a standard boundary element method (BEM), but into small arcs, while the linear part of the boundary divides into small segments. In such a case, the considered area can be described more accurately than when it divides into small segments, and as a result, a more accurate solution of the problem is obtained. Two test boundary-contact problems were solved by using a boundary element method developed in the polar coordinate system (PCSBEM), and the obtained numerical values are presented as tables and graphs.

\end{abstract}


\keywords{polar coordinates; elasticity problem; boundary element method; fictitious load method; boundary value problem.}

\begin{textblock*}{18cm}(1cm,1cm) % {block width} (coords) 
\textcolor{GJBlue}{\LARGE Global Journals \LaTeX\ JournalKaleidoscope\texttrademark}
\end{textblock*}

\begin{textblock*}{18cm}(1.4cm,1.5cm) % {block width} (coords) 
\textcolor{GJBlue}{\footnotesize \\ Artificial Intelligence formulated this projection for compatibility purposes from the original article published at Global Journals. However, this technology is currently in beta. \emph{Therefore, kindly ignore odd layouts, missed formulae, text, tables, or figures.}}
\end{textblock*}


\let\tabcellsep& 	 	 		 
\section[{I. Introduction}]{I. Introduction}\par
he boundary element method \hyperref[b0]{[1,}\hyperref[b1]{2]} is a helpful tool to solve the problems of computational mechanics. Many researchers and scientists use standard BEM, with the boundary approximation done by using linear segments (boundary elements), or standard BEM is improved by considering the conditions of a given problem \hyperref[b0]{[1]}\hyperref[b1]{[2]}\hyperref[b2]{[3]}\hyperref[b3]{[4]}\hyperref[b4]{[5]}\hyperref[b5]{[6]}\hyperref[b6]{[7]}\hyperref[b7]{[8]}\hyperref[b8]{[9]}\hyperref[b9]{[10]}\hyperref[b10]{[11]}\hyperref[b11]{[12]}\hyperref[b12]{[13]}\hyperref[b13]{[14]}\hyperref[b14]{[15]}\hyperref[b15]{[16]}\hyperref[b16]{[17]}\hyperref[b17]{[18]}\hyperref[b18]{[19]}. The advantage of using linear boundary elements is the opportunity to analytically calculate the integrals, while with curvilinear elements generally, it is possible to do numerical integration \hyperref[b19]{[20]}.\par
The boundary element method, in particular, the fictitious load method formulated to solve the boundary value and boundary-contact problems of elasticity for a circular ring and its parts are improved in the present paper if considering that the circular segment of the boundary is divided into arcs instead of linear segments. This allows to describe the considered area more accurately and to arrive at a more accurate solution of the problem. So, when the considered area is limited with circles or their parts, i.e., with the coordinate axes of the polar coordinate system, then by dividing the circle into small arcs, we can formulate BEM in the polar coordinate system with all integrals solved analytically. In particular, a fictitious load method is considered in the polar coordinate system, whereas it was described in a Cartesian coordinate system by Crouch and Star field \hyperref[b0]{[1]}.\par
The article gives a fundamental solution written down in polar coordinate systems serving as a basis to obtain a numerical solution, and a problem of constant forces distributed along the arc is considered. A numerical procedure is presented and boundary coefficients of influence are written out. Two test boundary-contact problems are solved: 1. Elastic equilibrium of an infinite area with a circular hole is studied when a circular ring inserts near the hole; normal constant stress is given on the internal surface of the ring, the body is free from stresses in the infinity, and the conditions of continuity of displacements and stresses are given on the contact line. Numerical values are obtained by using: a) analytical solution, b) standard BEM, i.e., when a circular boundary divides into linear segments, and c) PCSBEM, i.e., when the boundary divides into arcs, and the results obtained in all three cases are compared to one another. 2. A boundary-contact problem is solved for a doublelayer circular ring when the internal circular boundary is loaded with a normal variable force, the outer boundary is not loaded, and conditions of a rigid contact are given for the contact line. The numerical results are obtained by using standard BEM and PCSBEM and are compared to one another. MATLAB software was used to obtain the relevant numerical values and graphs for both problems. 
\section[{II. The Fundamental Solution in the Cartesian Coordinate System}]{II. The Fundamental Solution in the Cartesian Coordinate System}\par
Let us consider the problem shown in The solution to this problem is given by the following function \hyperref[b0]{[1]}:\par
where ? is the Poisson's ratio. The displacements will be written down as follows:\par
where( ) ? + = 1 2 E G\par
is shear modulus, and E is Young's modulus.\par
For the plane deformation, the stresses for Kelvin's problem will be written down as follows: ( ) ( ) [ ]\textbf{( ) ( ) ( ) [ ] ( ) ( ) [ ] ( )}[ ] . 2 1 2 1 , 1 2 2 , 2\textbf{1 2 , , , , , , , , , , , , , xy x}yg g F xg g F y x yg g F xg g F yg g F xg g F y x ? ? + ? ? = ? ? + ? = ? + ? ? = ? ? ? ? ? ? ? ? ?\par
As it can be seen from ( \hyperref[formula_2]{1}), \hyperref[b2]{(3)}, the stress at point 0 , 0 = = y x has the singularity. It can be shown that these stresses correspond to the point force at the origin of coordinates \hyperref[b20]{[21]}.\par
For the sake of simplicity, we mean that ( )y x i F F F , =\par
force is applied to the origin of coordinates. 
\section[{III. The Fundamental Solution in the Polar Coordinate System}]{III. The Fundamental Solution in the Polar Coordinate System}\par
Let us write down formulae (1), (  {\ref 2}) and (3) in \hyperref[b21]{[22]}. Following certain algebraic transformations, we obtain the following expression for the function ( )polar coordinate system ? , r ( ) ? ? 2 0 , 0 < ? ? < ? ry x g , : ( ) ( ) ( ) . ln 1 4 1 , , 1 r r g y x g ? ? ? ? ? = ?\par
For the components of a displacement vector, we will obtain the following equations:( ) ( ) [ ] ( ) ( ) ( ) ( ) [ ] sin 4 3 2 cos 2 , \textasciitilde , sin 2 cos 4 3 2 , \textasciitilde , 1 1 , 1 , 1 , 1 1 y y y x y x y x x x g r g G F g r G F r u g r G F g r g G F r u ? ? ? ? ? ? ? ? ? ? + ? = ? + ? ? =\par
and for the components of the stress tensor we will obtain:   ( ) ( ) [ ] ( ) ( ) ( ) ( ) [ ] ( ) ( ) [ ] ( ) [ ], sin 2 1 cos 2 1 , \textasciitilde  , sin 1 2 cos 2 , \textasciitilde , sin 2 cos 1 2 , \textasciitilde , 1 , 1 , 1\textbf{, 1 , 1 , 1 , 1 , 1 , 1 , 1 , 1 ,}g r g F g r g F r g r g F g r g F r g r g F g r g F r ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? + ? ? = ? ? + ? = ? + ? ? = ( ) ( ) ( ) , ln 1 4 1 , 2 2 y x y x g + ? ? = ? ?? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? = ? ? = ? = ? ? = ? ? =\par
By using the superposition principle, we can solve the problem for an infinite elastic body, with a set of point forces acting at any of its points. If distributing such forces continuously along some line of the plane, we will obtain a problem with the forces given along this line. 
\section[{IV. Constant Forces Distributed the Curve}]{IV. Constant Forces Distributed the Curve}\par
Let us consider the following problem: constant    ( ) ( )( ) ( ) [ \{ ( ) ( ) ( ) ( ) ( )] ( ) ( ) ( ) ( )\} ( ) ( ) ( ) ( ) ( ) ( ) \{ ( )( ) [ ( ) ( ) ( ) ( ) ( ) ( )]\},2 1 2 1 2 1 2 2 1 2 1 2 1 2 1 2 ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? + ? + ? ? ? + ? ? ? ? ? = ? ? ? ? ? + ? + ? + ? ? ? = r P P G r u P r P G( ) ( ) ( ) ( ) ( ) [ \{ ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) [ \{ ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) ( ) ( )\textbf{( ) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) ( ) (}\par
) .    {\ref 6}) and (  {\ref 7}) are displacements and stresses in an infinite elastic body when constant2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 ? ? ? ? ? ? ? ? ? ? ? ? ? ? + ? ? ? ? ? ? + ? ? ? ? ? ? = ? ? ? ? ? ? ? ? ? + ? ? ? ? ? ? ? ? ? ? ? + ? ? ? ? ? ? = ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? = ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ?r r P t = and ? ? P t = forces are applied to 2 1 ? ? ? ? ?\par
arc of a circle with the radius r . These equations are the basis for the boundary element method considered later. The following peculiarity of the analytical solution given above is worth mentioning. Displacements from the origin of coordinates to the infinitely distanced points are not limited because of the logarithm included in them. Therefore, equations \hyperref[b5]{(6)} show only relative displacements. In any concrete case, we must choose a reference point and determine the displacement in respect of such a point. 
\section[{V. Numerical Procedure}]{V. Numerical Procedure}\par
The analytical solution obtained above is the basis for the boundary element method used to obtain a numerical solution of the boundary value problem of the theory of elasticity. Let us explain the physical aspect of this method by using a specific example. Let us consider a boundary value problem for an infinite body with a hole (with a circular hole in our case). We will consider a plane deformation. Let us denote the boundary of the cut, which is a circle in our case, by C (See Fig. \hyperref[fig_8]{3}). At any point of the C curve, local s and n coordinates have the direction of a tangent and its perpendicular. Therefore, they change at different points along the border. We take these coordinates so that the direction of n should coincide with the direction of an outer normal at the same point as the border and s should coincide with the direction of the boundary line. In this case, the direction of the boundary line is anticlockwise. Let us assume that the same normal stress ( the whole length of every element, and the tangent is free from stress. In this case, the boundary conditions will be as follows:( ). , 1 , 0 , N i p i s i n ? = = ? = ? ?\par
Let us imagine that constant normal and tangent stresses act on every element of the circle, e.g., let us denote the normal and tangent stresses acting on the element j by j n P and j s P , respectively.\par
It should be noted that the real normal and tangent tresses acting on the element j do not equal to j n P and j s P , if stresses act on other elements, too.\par
Therefore, there are two different kinds of stresses for every element. For example, for the element j , we have applied stresses ) applied to the element j .\par
By considering the boundary conditions, we will obtain the following equations:  It should be noted that j n P and j s P stresses in these equations are fictitious values. They are introduced as an intermediate quantity to obtain the numerical value of the problem, and they have no physical essence. However, a linear combination of a fictitious load presented with formulae (8) has a physical essence in the considered problem, and is the basis to obtain a system of algebraic equations \hyperref[b8]{(9)}. After solving this system, we can express displacements and stresses at any point in a body with another combination of j n P and j s P , ( N j ? , 1 =\par
) fictitious load.\par
The above-described boundary element method is called a fictitious load method \hyperref[b0]{[1]}. 
\section[{VI. Influence Coefficients}]{VI. Influence Coefficients}\par
Let us write down the expressions of the tangent and normal displacements and stresses in the middle point of the i -th element caused by fictitious loads j n P and j s P , N j ? , 1 = applied to the j -th element. For the displacements, we will have:     wher e r and ? are coordinates in the local coordinate system, with its center coinciding with the middle point of the i -th element. Generally, the displacements and stresses in the i -th element are functions of the j s P and j n P fictitious load on all N elements. So, by \hyperref[b9]{(10)} and \hyperref[b10]{(11)}, we can write down:   {\ref 10}) and \hyperref[b10]{(11)}. For example, the ij sn A coefficient is calculated with the expression given in curly braces at j n P of the first equation of \hyperref[b9]{(10)}.( ) ( )( ) ( ) [ ( ) ( ) ( ) ( )]\} ( ) ( ) ( ) ( ) ( ) [ ] ( ) ( ) ( ) ( ) ( ) [ ]\textbf{( ) ( )( ) ( ) [ ( ) ( ) ( ) ( ) ( )]\}}2 1 2 1 2 1 2 2 1 2 2 1 2 2 1 2 1 2 1 2 ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? + ? ? ? ? ? ? ? ? ? ? ? = ? ? ? ? ? ? ? ? ? ? ? + ? ? ? + ? ? ? ? + ? ? ? =) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) (\textbf{) ( ) ( ) ( ) ( ) ( ) ( ) [ ( ) ( ) ( ) ( ) ( ) , 3}2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 2 1 ? ? ? ? ? ? ? ? ? + ? ? ? ? ? ? ? ? + ? ? ? ? ? ? ? ? ? + ? ? ? ? ? ? ? ? ? = ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? + ? ? ? ? ? ? ? ? ? + ? ? ? ? ? ? ? ? ? = ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? + ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? = ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ? ?( ) ( ) , ,\textbf{1 1 ? ?} 
\section[{VII. Numerical Examples and Discussion}]{VII. Numerical Examples and Discussion}\par
There are two test problems of using a fictitious load method given below. We have an exact solution to one problem. Therefore, in the case of dividing the boundary into segments and arcs, the numerical results obtained by using the boundary element method will be compared to the exact values. Another problem will compare the numerical values obtained by using the fictitious load method to one another in case of dividing the boundary into segments on the one hand and into arcs on the other hand. and for the stresses, the expressions will be as follows: E as its elastic characteristics (See Fig. 4). p rr ? = ? normal stress is given on the internal surface of the ring, while in the infinity, the body is free from stresses, and the continuity conditions of displacements and stresses are given on b r = contact surface. So, we will have the following boundary conditions: ( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) . , , , : 2 1 2 1 2 1 2 1 ? ? ? ? ? ? ? ? u u u u b r r r r r rr rr ? = ? = = = =\par
The solution to this problem is obtained from standard formulae \hyperref[b22]{[23,}\hyperref[b23]{24]} for a thick-wall cylinder. In particular, the radial and tangential stresses are calculated with the following formulae \hyperref[b0]{[1]}: surface are divided into n=90 elements each, and the obtained visual and numerical results are presented in Fig. 5, Fig. 6, Table \hyperref[tab_4]{1 and Table 2}, while in cases shown in Fig. 7, Fig. 8, Table \hyperref[tab_9]{3 and Table 4}, they are divided into 180 elements each.            9. This problem, too, is symmetrical to both coordinate axes and therefore, we will consider it for a one-fourth of a circular ring. So, the area to be considered is2 1 ? + ? = ? ,where ? ? ? ? ? ? ? ? ? ? = ? 2 0 , 1 ? ? b r a , ? ? ? ? ? ? ? ? ? ? = ? 2 0 , 2 ? ? c r b .\par
The boundary conditions will be written down as follows: The conditions of a rigid contact will be written down as follows:      \hyperref[tab_4]{2}, when n=90 and Fig. 8, Table \hyperref[tab_7]{4}, when n=180), is almost twice as less in terms of percents. It should be noted that in case of dividing the boundary into very small elements, e.g., when n=180, the error is more, as the arithmetic operations with very small numbers results in additional errors (counter error).( ) ( ) ( ) ( ) ( ) ( ) ( ) ( ) . , , , :\par
Paragraph 7.2 considers the boundary-contact problem for a double-layer circular ring with a normal 
\section[{VIII. Conclusion}]{VIII. Conclusion}\par
The article develops BEM, in particular, the fictitious load method in the polar coordinate system (PCSBEM) to solve the boundary value and boundarycontact problems of the theory of elasticity for the areas limited by the coordinate axes of a polar coordinate system. The bodies relevant to such areas are quite frequent in practice, e.g., in building the underground structures (tunnels), in mechanical engineering, etc. Consequently, the above-described method (PCSBEM) is one of the means to obtain the adjusted solutions of the problems of computational mechanics, as the boundary of the considered area is divided not into small segments, like in case of a standard boundary element method (BEM), but into small arcs. In this case, the boundary of the considered area can be described more accurately, and consequently, the solution to the problem will be more accurate. To illustrate this case, two test boundary-contact problems are solved by using standard BEM and PCSBEM. The obtained numerical results given as tables and graphs are analyzed in paragraph 7.  \hyperref[tab_8]{5}, where one can see that they coincide with one another quite exactly.\begin{figure}[htbp]
\noindent\textbf{}\includegraphics[]{image-2.png}
\caption{\label{fig_0}}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{1}\includegraphics[]{image-3.png}
\caption{\label{fig_1}Figure 1 :}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{}\includegraphics[]{image-4.png}
\caption{\label{fig_2}}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{2}\includegraphics[]{image-5.png}
\caption{\label{fig_3}Figure 2 :F}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{}\includegraphics[]{image-6.png}
\caption{\label{fig_5}}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{3}\includegraphics[]{image-7.png}
\caption{\label{fig_8}Figure 3 :}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{}\includegraphics[]{image-8.png}
\caption{\label{fig_9}?}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{}\includegraphics[]{image-9.png}
\caption{\label{fig_11}}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{}\includegraphics[]{image-10.png}
\caption{\label{fig_13}J}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{}\includegraphics[]{image-11.png}
\caption{\label{fig_14}(}\end{figure}
             \begin{figure}[htbp]
\noindent\textbf{1} \par 
\begin{longtable}{P{0.028523489932885907\textwidth}P{0.10458612975391499\textwidth}P{0.0009507829977628635\textwidth}P{0.11694630872483221\textwidth}P{0.001901565995525727\textwidth}P{0.04278523489932885\textwidth}P{0.0009507829977628635\textwidth}P{0.13215883668903802\textwidth}P{0.0047539149888143175\textwidth}P{0.0009507829977628635\textwidth}P{0.03422818791946308\textwidth}P{0.0009507829977628635\textwidth}P{0.0009507829977628635\textwidth}P{0.11884787472035795\textwidth}P{0.1378635346756152\textwidth}P{0.0028523489932885905\textwidth}P{0.11314317673378077\textwidth}P{0.0009507829977628635\textwidth}P{0.005704697986577181\textwidth}}
\tabcellsep \tabcellsep \tabcellsep ?\tabcellsep ??\tabcellsep /\tabcellsep p\tabcellsep in the ring\tabcellsep 5 . 0\tabcellsep ?\tabcellsep b r\tabcellsep ?\tabcellsep 1\tabcellsep \multicolumn{2}{l}{and infinite body}\tabcellsep b r\tabcellsep ?\tabcellsep 1\tabcellsep (n=90)\\
\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{7}{l}{Approximate solution}\tabcellsep \multicolumn{2}{l}{Relative error, percent}\\
No.\tabcellsep r /\tabcellsep b\tabcellsep Exact solution\tabcellsep \tabcellsep \multicolumn{4}{l}{In case of the division into segments}\tabcellsep \tabcellsep \multicolumn{4}{l}{In case of the division into arcs}\tabcellsep \multicolumn{2}{l}{Segments}\tabcellsep Arcs\\
1\tabcellsep \multicolumn{2}{l}{0.5500}\tabcellsep 1.0294\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.9726\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 1.0010\tabcellsep \multicolumn{2}{l}{5.5160}\tabcellsep 2.7574\\
2\tabcellsep \multicolumn{2}{l}{0.6000}\tabcellsep 0.8827\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.8446\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.8637\tabcellsep \multicolumn{2}{l}{4.3169}\tabcellsep 2.1543\\
3\tabcellsep \multicolumn{2}{l}{0.6500}\tabcellsep 0.7686\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.7437\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.7561\tabcellsep \multicolumn{2}{l}{3.2348}\tabcellsep 1.6174\\
4\tabcellsep \multicolumn{2}{l}{0.7000}\tabcellsep 0.6780\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.6621\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.6701\tabcellsep \multicolumn{2}{l}{2.3412}\tabcellsep 1.1706\\
5\tabcellsep \multicolumn{2}{l}{0.7500}\tabcellsep 0.6049\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.5950\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.6000\tabcellsep \multicolumn{2}{l}{1.6392}\tabcellsep 0.8196\\
6\tabcellsep \multicolumn{2}{l}{0.8000}\tabcellsep 0.5451\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.5392\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.5422\tabcellsep \multicolumn{2}{l}{1.0956}\tabcellsep 0.5478\\
7\tabcellsep \multicolumn{2}{l}{08500}\tabcellsep 0.4956\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.4923\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.4939\tabcellsep \multicolumn{2}{l}{0.6601}\tabcellsep 0.3300\\
8\tabcellsep \multicolumn{2}{l}{0.9000}\tabcellsep 0.4540\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.4528\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.4534\tabcellsep \multicolumn{2}{l}{0.2769}\tabcellsep 0.1395\\
9\tabcellsep \multicolumn{2}{l}{0.9500}\tabcellsep 0.4189\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.4194\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.4191\tabcellsep \multicolumn{2}{l}{0.1096}\tabcellsep 0.0548\\
10\tabcellsep \multicolumn{2}{l}{1.0500}\tabcellsep 0.1512\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1507\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1509\tabcellsep \multicolumn{2}{l}{0.3242}\tabcellsep 0.1621\\
11\tabcellsep \multicolumn{2}{l}{1.1000}\tabcellsep 0.1377\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1370\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1374\tabcellsep \multicolumn{2}{l}{0.5607}\tabcellsep 0.2803\\
12\tabcellsep \multicolumn{2}{l}{1.1500}\tabcellsep 0.1260\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1250\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1255\tabcellsep \multicolumn{2}{l}{0.7963}\tabcellsep 0.3981\\
13\tabcellsep \multicolumn{2}{l}{1.2000}\tabcellsep 0.1157\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1146\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1151\tabcellsep \multicolumn{2}{l}{1.0238}\tabcellsep 0.5119\\
14\tabcellsep \multicolumn{2}{l}{1.2500}\tabcellsep 0.1067\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1053\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1060\tabcellsep \multicolumn{2}{l}{1.2381}\tabcellsep 0.6192\\
15\tabcellsep \multicolumn{2}{l}{1.3000}\tabcellsep 0.0986\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0972\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0979\tabcellsep \multicolumn{2}{l}{1.4361}\tabcellsep 0.7181\\
16\tabcellsep \multicolumn{2}{l}{1.3500}\tabcellsep 0.0914\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0900\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0907\tabcellsep \multicolumn{2}{l}{1.6165}\tabcellsep 0.8083\\
17\tabcellsep \multicolumn{2}{l}{1.4000}\tabcellsep 0.0850\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0835\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0843\tabcellsep \multicolumn{2}{l}{1.7787}\tabcellsep 0.8894\\
18\tabcellsep \multicolumn{2}{l}{1.4500}\tabcellsep 0.0793\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0777\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0785\tabcellsep \multicolumn{2}{l}{1.9234}\tabcellsep 0.9714\\
\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{3}{l}{Average}\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{1.6605}\tabcellsep 0.8306\end{longtable} \par
 
\caption{\label{tab_3}Table 1 :}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{2} \par 
\begin{longtable}{P{0.049999999999999996\textwidth}P{0.19999999999999998\textwidth}P{0.049999999999999996\textwidth}P{0.55\textwidth}}
?\tabcellsep rr /\tabcellsep p\tabcellsep in the ring\end{longtable} \par
 
\caption{\label{tab_4}Table 2 :}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{3} \par 
\begin{longtable}{P{0.02849162011173184\textwidth}P{0.10446927374301675\textwidth}P{0.0009497206703910614\textwidth}P{0.11681564245810055\textwidth}P{0.0018994413407821228\textwidth}P{0.007597765363128491\textwidth}P{0.03608938547486033\textwidth}P{0.13201117318435754\textwidth}P{0.0047486033519553075\textwidth}P{0.0009497206703910614\textwidth}P{0.002849162011173184\textwidth}P{0.03229050279329609\textwidth}P{0.1035195530726257\textwidth}P{0.016145251396648044\textwidth}P{0.1377094972067039\textwidth}P{0.002849162011173184\textwidth}P{0.1130167597765363\textwidth}P{0.0009497206703910614\textwidth}P{0.0066480446927374304\textwidth}}
\tabcellsep \tabcellsep \tabcellsep ?\tabcellsep ??\tabcellsep /\tabcellsep p\tabcellsep in the ring\tabcellsep 5 . 0\tabcellsep ?\tabcellsep b r\tabcellsep ?\tabcellsep 1\tabcellsep \multicolumn{2}{l}{and infinite body}\tabcellsep b r\tabcellsep ?\tabcellsep 1\tabcellsep (n=180)\\
\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{6}{l}{Approximate solution}\tabcellsep \tabcellsep \multicolumn{2}{l}{Relative error, percent}\\
No.\tabcellsep r /\tabcellsep b\tabcellsep Exact solution\tabcellsep \tabcellsep \tabcellsep \multicolumn{3}{l}{In case of the division into segments}\tabcellsep \tabcellsep \tabcellsep \multicolumn{3}{l}{In case of the division into arcs}\tabcellsep \multicolumn{2}{l}{Segments}\tabcellsep Arcs\\
1\tabcellsep \multicolumn{2}{l}{0.5500}\tabcellsep 1.0294\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.9895\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{1.0095}\tabcellsep \multicolumn{2}{l}{3.8708}\tabcellsep 1.9317\\
2\tabcellsep \multicolumn{2}{l}{0.6000}\tabcellsep 0.8827\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.8539\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.8683}\tabcellsep \multicolumn{2}{l}{3.2648}\tabcellsep 1.6331\\
3\tabcellsep \multicolumn{2}{l}{0.6500}\tabcellsep 0.7686\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.7475\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.7580}\tabcellsep \multicolumn{2}{l}{2.7475}\tabcellsep 1.3757\\
4\tabcellsep \multicolumn{2}{l}{0.7000}\tabcellsep 0.6780\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.6622\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.6701}\tabcellsep \multicolumn{2}{l}{2.3276}\tabcellsep 1.1659\\
5\tabcellsep \multicolumn{2}{l}{0.7500}\tabcellsep 0.6049\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.5960\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.6005}\tabcellsep \multicolumn{2}{l}{1.4713}\tabcellsep 0.7274\\
6\tabcellsep \multicolumn{2}{l}{0.8000}\tabcellsep 0.5451\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.5400\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.5445}\tabcellsep \multicolumn{2}{l}{0.9356}\tabcellsep 0.1101\\
7\tabcellsep \multicolumn{2}{l}{08500}\tabcellsep 0.4956\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.4930\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.4940}\tabcellsep \multicolumn{2}{l}{0.5246}\tabcellsep 0.3228\\
8\tabcellsep \multicolumn{2}{l}{0.9000}\tabcellsep 0.4540\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.4531\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.4536}\tabcellsep \multicolumn{2}{l}{0.1982}\tabcellsep 0.0881\\
9\tabcellsep \multicolumn{2}{l}{0.9500}\tabcellsep 0.4189\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.4183\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.4185}\tabcellsep \multicolumn{2}{l}{0.1432}\tabcellsep 0.0955\\
10\tabcellsep \multicolumn{2}{l}{1.0500}\tabcellsep 0.1512\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1509\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.1510}\tabcellsep \multicolumn{2}{l}{0.1984}\tabcellsep 0.1323\\
11\tabcellsep \multicolumn{2}{l}{1.1000}\tabcellsep 0.1377\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1372\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.1375}\tabcellsep \multicolumn{2}{l}{0.3631}\tabcellsep 0.1452\\
12\tabcellsep \multicolumn{2}{l}{1.1500}\tabcellsep 0.1260\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1252\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.1256}\tabcellsep \multicolumn{2}{l}{0.6349}\tabcellsep 0.3175\\
13\tabcellsep \multicolumn{2}{l}{1.2000}\tabcellsep 0.1157\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1150\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.1154}\tabcellsep \multicolumn{2}{l}{0.6050}\tabcellsep 0.2593\\
14\tabcellsep \multicolumn{2}{l}{1.2500}\tabcellsep 0.1067\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.1058\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.1062}\tabcellsep \multicolumn{2}{l}{0.8435}\tabcellsep 0.4686\\
15\tabcellsep \multicolumn{2}{l}{1.3000}\tabcellsep 0.0986\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0978\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.0983}\tabcellsep \multicolumn{2}{l}{0.3043}\tabcellsep 0.8114\\
16\tabcellsep \multicolumn{2}{l}{1.3500}\tabcellsep 0.0914\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0907\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.0912}\tabcellsep \multicolumn{2}{l}{0.7659}\tabcellsep 0.2188\\
17\tabcellsep \multicolumn{2}{l}{1.4000}\tabcellsep 0.0850\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0844\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.0847}\tabcellsep \multicolumn{2}{l}{0.7059}\tabcellsep 0.2353\\
18\tabcellsep \multicolumn{2}{l}{1.4500}\tabcellsep 0.0793\tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.0788\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{0.0791}\tabcellsep \multicolumn{2}{l}{0.6305}\tabcellsep 0.2522\\
\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{3}{l}{Average}\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{2}{l}{1.1408}\tabcellsep 0.5717\end{longtable} \par
 
\caption{\label{tab_6}Table 3 :}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{4} \par 
\begin{longtable}{P{0.09508196721311475\textwidth}P{0.09016393442622951\textwidth}P{0.000819672131147541\textwidth}P{0.11557377049180328\textwidth}P{0.03934426229508197\textwidth}P{0.000819672131147541\textwidth}P{0.12950819672131147\textwidth}P{0.004098360655737705\textwidth}P{0.000819672131147541\textwidth}P{0.029508196721311473\textwidth}P{0.000819672131147541\textwidth}P{0.000819672131147541\textwidth}P{0.11721311475409836\textwidth}P{0.021311475409836064\textwidth}P{0.10081967213114754\textwidth}P{0.09754098360655737\textwidth}P{0.005737704918032787\textwidth}}
\tabcellsep \tabcellsep \tabcellsep ?\tabcellsep rr /\tabcellsep p\tabcellsep in the ring\tabcellsep 5 . 0\tabcellsep ?\tabcellsep b r\tabcellsep ?\tabcellsep 1\tabcellsep and infinite body\tabcellsep b r\tabcellsep ?\tabcellsep 1\tabcellsep (n=180)\\
\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{7}{l}{Approximate solution}\tabcellsep \multicolumn{2}{l}{Relative error, percent}\\
No.\tabcellsep r /\tabcellsep b\tabcellsep Exact solution\tabcellsep \multicolumn{4}{l}{In case of the division into segments}\tabcellsep \tabcellsep \multicolumn{4}{l}{In case of the division into arcs}\tabcellsep \tabcellsep Segments\tabcellsep Arcs\\
1\tabcellsep \multicolumn{2}{l}{0.5500}\tabcellsep -0.8072\tabcellsep \tabcellsep \tabcellsep -0.8124\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.8098\tabcellsep \tabcellsep 0.6519\tabcellsep 0.3268\\
2\tabcellsep \multicolumn{2}{l}{0.6000}\tabcellsep -0.6605\tabcellsep \tabcellsep \tabcellsep -0.6675\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.6640\tabcellsep \tabcellsep 1.0552\tabcellsep 0.5308\\
3\tabcellsep \multicolumn{2}{l}{0.6500}\tabcellsep -0.5464\tabcellsep \tabcellsep \tabcellsep -0.5535\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.5499\tabcellsep \tabcellsep 1.3036\tabcellsep 0.6496\\
4\tabcellsep \multicolumn{2}{l}{0.7000}\tabcellsep -0.4558\tabcellsep \tabcellsep \tabcellsep -0.4622\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.4590\tabcellsep \tabcellsep 1.4077\tabcellsep 0.7060\\
5\tabcellsep \multicolumn{2}{l}{0.7500}\tabcellsep -0.3827\tabcellsep \tabcellsep \tabcellsep -0.3880\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.3854\tabcellsep \tabcellsep 1.3926\tabcellsep 0.7013\\
6\tabcellsep \multicolumn{2}{l}{0.8000}\tabcellsep -0.3229\tabcellsep \tabcellsep \tabcellsep -0.3271\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.3250\tabcellsep \tabcellsep 1.2871\tabcellsep 0.6452\\
7\tabcellsep \multicolumn{2}{l}{08500}\tabcellsep -0.2734\tabcellsep \tabcellsep \tabcellsep -0.2764\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.2749\tabcellsep \tabcellsep 1.1177\tabcellsep 0.5647\\
8\tabcellsep \multicolumn{2}{l}{0.9000}\tabcellsep -0.2318\tabcellsep \tabcellsep \tabcellsep -0.2339\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.2329\tabcellsep \tabcellsep 0.9077\tabcellsep 0.4640\\
9\tabcellsep \multicolumn{2}{l}{0.9500}\tabcellsep -0.1967\tabcellsep \tabcellsep \tabcellsep -0.1980\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.1973\tabcellsep \tabcellsep 0.6761\tabcellsep 0.3173\\
10\tabcellsep \multicolumn{2}{l}{1.0500}\tabcellsep -0.1512\tabcellsep \tabcellsep \tabcellsep -0.1522\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.1517\tabcellsep \tabcellsep 0.6921\tabcellsep 0.3496\\
11\tabcellsep \multicolumn{2}{l}{1.1000}\tabcellsep -0.1377\tabcellsep \tabcellsep \tabcellsep -0.1383\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.1380\tabcellsep \tabcellsep 0.4447\tabcellsep 0.1880\\
12\tabcellsep \multicolumn{2}{l}{1.1500}\tabcellsep -0.1260\tabcellsep \tabcellsep \tabcellsep -0.1263\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.1262\tabcellsep \tabcellsep 0.2216\tabcellsep 0.1397\\
13\tabcellsep \multicolumn{2}{l}{1.2000}\tabcellsep -0.1157\tabcellsep \tabcellsep \tabcellsep -0.1158\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.1158\tabcellsep \tabcellsep 0.0207\tabcellsep 0.0512\\
14\tabcellsep \multicolumn{2}{l}{1.2500}\tabcellsep -0.1067\tabcellsep \tabcellsep \tabcellsep -0.1065\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.1066\tabcellsep \tabcellsep 0.1600\tabcellsep 0.0625\\
15\tabcellsep \multicolumn{2}{l}{1.3000}\tabcellsep -0.0986\tabcellsep \tabcellsep \tabcellsep -0.0983\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.0985\tabcellsep \tabcellsep 0.3226\tabcellsep 0.1210\\
16\tabcellsep \multicolumn{2}{l}{1.3500}\tabcellsep -0.0914\tabcellsep \tabcellsep \tabcellsep -0.0910\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.0912\tabcellsep \tabcellsep 0.4690\tabcellsep 0.2728\\
17\tabcellsep \multicolumn{2}{l}{1.4000}\tabcellsep -0.0850\tabcellsep \tabcellsep \tabcellsep -0.08.45\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.0848\tabcellsep \tabcellsep 0.6011\tabcellsep 0.2752\\
18\tabcellsep \multicolumn{2}{l}{1.4500}\tabcellsep -0.0793\tabcellsep \tabcellsep \tabcellsep -0.0787\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep -0.0790\tabcellsep \tabcellsep 0.7203\tabcellsep 0.3415\\
\tabcellsep \tabcellsep \tabcellsep \tabcellsep \multicolumn{3}{l}{Average}\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep 0.7473\tabcellsep 0.3726\\
\multicolumn{4}{l}{b) Double-layer circular ring}\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \\
\multicolumn{7}{l}{Let us consider the boundary-contact problem}\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \\
\multicolumn{2}{l}{shown in Fig.}\tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \tabcellsep \end{longtable} \par
 
\caption{\label{tab_7}Table 4 :}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{5} \par 
\begin{longtable}{P{0.6710526315789473\textwidth}P{0.13421052631578947\textwidth}P{0.04473684210526315\textwidth}}
? on the circle\tabcellsep r =\tabcellsep a\end{longtable} \par
 
\caption{\label{tab_8}Table 5 :}\end{figure}
 \begin{figure}[htbp]
\noindent\textbf{3} \par 
\begin{longtable}{}
\end{longtable} \par
 
\caption{\label{tab_9}Table 3 ,}\end{figure}
 			\footnote{© 2018 Global Journals} 			\footnote{J© 2018 Global Journals} 			\footnote{J © 2018 Global Journals Development of Boundary Element Method in Polar Coordinate System for Elasticity Problems} 			\footnote{Development of Boundary Element Method in Polar Coordinate System for Elasticity Problems © 2018 Global Journals} 		 		\backmatter  			  				\begin{bibitemlist}{1}
\bibitem[Tsiatas ()]{b14}\label{b14} 	 		‘A BEM-based meshless solution to buckling problems of orthotropic plates’.  		 			G C Tsiatas 		,  		 			YiotisA 		.  	 	 		\textit{Engineering Analysis with Boundary Elements}  		2013. 37 p. .  	 
\bibitem[Zhao Liu Yijun et al. ()]{b16}\label{b16} 	 		‘A fast multipole boundary element method for modeling 2-D multiple crack problems with constant elements’.  		 			Guo Zhao Liu Yijun 		,  		 			Ma Hang 		,  		 			Huang Shuo 		.  	 	 		\textit{Engineering Analysis with Boundary Elements}  		2014. 47 p. .  	 
\bibitem[Ahmed and Meshrif ()]{b8}\label{b8} 	 		‘A new numerical algorithm for 2D moving boundary problems using a boundary element method’.  		 			S G Ahmed 		,  		 			S A Meshrif 		.  	 	 		\textit{Computers and Mathematics with Applications}  		2009. 2018. 58 p. .  	 	 (Volume XVIII Issue V Version I Year) 
\bibitem[Riccardela ()]{b2}\label{b2} 	 		\textit{An implementation of the boundary-integral technique for planar problems of elasticity and elasto-plasticity},  		 			P C Riccardela 		.  		1973.  		 			Carnegie Mellon University 		 	 	 (Ph.D. thesis) 
\bibitem[Potapenko ()]{b18}\label{b18} 	 		‘An integral representation for the solution of the inclusion problem in the theory of antiplane micropolar elasticity’.  		 			S Potapenko 		.  		 \xref{http://dx.doi.org/10.1177/1081286516680861}{10.1177/1081286516680861}.  		 \url{https://doi.org/10.1177/1081286516680861}  	 	 		\textit{Mathematics and Mechanics Solids}  		2016. 23  (4)  p. .  	 
\bibitem[Zirakashvili ()]{b5}\label{b5} 	 		‘Application of the boundary element method to the solution of the problem of distribution of stresses in an elastic body with a circular hole whose interior surface contains radial cracks’.  		 			N Zirakashvili 		.  	 	 		\textit{Proceedings of A.Razmadze Mathematical Institute}  		2006. 141 p. .  	 
\bibitem[W?cel ()]{b3}\label{b3} 	 		‘BEM-FVM solution of the conjugate radiative and convective heat transfer problem’.  		 			G W?cel 		.  	 	 		\textit{Archives of Computational Methods in Engineering}  		2006. 13  (2)  p. .  	 
\bibitem[Mohammadi et al. ()]{b11}\label{b11} 	 		‘Boundary element analysis of thermo-elastic problems with non-uniform heat sources’.  		 			M Mohammadi 		,  		 			M R Hematiyan 		,  		 			M Aliabadi 		.  	 	 		\textit{The Journal of Strain Analysis for Engineering Design}  		2010. 45  (8)  p. .  	 
\bibitem[Crouch and Starfield ()]{b0}\label{b0} 	 		‘Boundary element methods in solid mechanics’.  		 			S L Crouch 		,  		 			A M Starfield 		.  	 	 		\textit{George Allen \& Unwin}  		1983.  	 
\bibitem[Brebbia et al. ()]{b1}\label{b1} 	 		\textit{Boundary element techniques: theory and applications in engineering},  		 			C A Brebbia 		,  		 			J F Telles 		,  		 			L C Wrobel 		.  		1984. Berlin Heidelberg New York Tokyo: Springer-Verlag.  	 
\bibitem[Song and Yinglong ()]{b6}\label{b6} 	 		‘Comparison of the BEM and DRBEM in solving the Helmholtz equation’.  		 			Zhu Song 		,  		 			-Ping 		,  		 			Zhang Yinglong 		.  	 	 		\textit{ANZIAM J}  		2007. 49 p. .  	 
\bibitem[Lachat and Watson ()]{b19}\label{b19} 	 		‘Effective numerical treatment of boundary-integral equations: a formulation for tree-dimensional elastostatics’.  		 			J C Lachat 		,  		 			J O Watson 		.  	 	 		\textit{Int. J. Num. Methods Eng}  		1976. 10 p. .  	 
\bibitem[Jaeger ()]{b22}\label{b22} 	 		\textit{Elasticity, fracture and flow, with engineering and geological applications},  		 			J C Jaeger 		.  		1962. London.  	 	 (2nd edn.) 
\bibitem[Yua]{b23}\label{b23} 	 		\textit{Konyaeva M (translator) (1979) Theory of elasticity},  		 			Amenzade Yua 		.  		Moscow: Mir Publishers.  	 	 (in Russian) 
\bibitem[Bermant ()]{b21}\label{b21} 	 		\textit{Mapping linear coordinates. Transformation. Green's formulas},  		 			A F Bermant 		.  		1958. Moscow: Fizmatgiz.  	 	 (in Russian) 
\bibitem[Chen et al. ()]{b4}\label{b4} 	 		‘Mathematical analysis and numerical study to free vibrations of annular plates using BIEM and BEM’.  		 			J T Chen 		,  		 			Lin Sy 		,  		 			Chen I L Lee 		,  		 			YT 		.  	 	 		\textit{Int. J. Numer. Meth}  		2006. 65 p. .  	 
\bibitem[Zirakashvili ()]{b7}\label{b7} 	 		‘Numerical Analysis of the Stress Distribution by the Boundary Elements Method in Continuous Body with a Hole’.  		 			N Zirakashvili 		.  	 	 		\textit{Bull. Georg. Nat. Acad. Sci}  		2007. 175  (3)  p. .  	 
\bibitem[Zirakashvili ()]{b9}\label{b9} 	 		‘Numerical Solution of Some Plane Boundary Value Problems of the Theory of Binary Mixtures by the Boundary Element Method’.  		 			N Zirakashvili 		,  		 			Janjgava 		.  	 	 		\textit{Applied Mathematics Informatics and Mechanics}  		2009. 14  (1)  p. .  	 
\bibitem[Zirakashvili ()]{b15}\label{b15} 	 		‘On the numerical solution of some two-dimensional boundary-contact delocalization problems’.  		 			N Zirakashvili 		.  	 	 		\textit{Meccanica}  		2013. 48  (7)  p. .  	 
\bibitem[Khomasuridze and Zirakashvili ()]{b12}\label{b12} 	 		‘Strain control of cracked elasic bodies means of boundary condition variation’.  		 			N Khomasuridze 		,  		 			N Zirakashvili 		.  	 	 		\textit{Proceedings of International Conference "Architecture and Construction -Contemporary Problems},  				 (International Conference "Architecture and Construction -Contemporary ProblemsYerevan -Jermuk)  		2010. p. .  	 
\bibitem[Zirakashvili ()]{b13}\label{b13} 	 		‘Study of stress-strain state of the piecewise homogeneous elastic body. Reports of Enlarged Session of the Seminar of I’.  		 			N Zirakashvili 		.  	 	 		\textit{Vekua Institute of Applied Mathematics}  		2010. 24 p. .  	 
\bibitem[Zirakashvili ()]{b10}\label{b10} 	 		‘The numerical solution of boundary-value problems for an elastic body with an elliptic hole and linear cracks’.  		 			N Zirakashvili 		.  	 	 		\textit{Journal of Engineering Mathematics}  		2009. 65  (2)  p. .  	 
\bibitem[Timoshenko and Goodier ()]{b20}\label{b20} 	 		\textit{Theory of elasticity. 3 rd edn},  		 			S P Timoshenko 		,  		 			J N Goodier 		.  		1970. New York: McGraw-Hill.  	 
\bibitem[Morcos et al. ()]{b17}\label{b17} 	 		\textit{Youssef F. Rashed, Taylor series fast multipole boundary element method for solution of Reissner's shear deformable plate bending problems. Engineering Analysis with Boundary Elements},  		 			F Morcos 		,  		 			Mohammed E Samaan 		,  		 			Nassar 		.  		2015. 59 p. .  	 
\end{bibitemlist}
 			 		 	 
\end{document}
